1. **Stand on the destination location to copied the files**
2. **ftp to the source server**

ilhp053!mb\_cctsa:/sdkhome/sdk/Installation\_Files/ABP7.5/SP1/PB18/7.5.1.18.41 [89]> ftp hpx612a

Connected to hpx612a.corp.amdocs.com.

220 hpx612a.corp.amdocs.com FTP server (Revision 1.1 Version wuftpd-2.6.1(PHNE\_34698) Fri Nov 10 10:21:03 GMT 2006) ready.

Name (hpx612a:mb\_cctsa): apsdlv

331 Password required for apsdlv.

Password:

230 User apsdlv logged in.

Remote system type is UNIX.

Using binary mode to transfer files.

1. **Go the source files in the server**

ftp> cd /APS/delivery/v750/SP1/HP/PatchBundle/PB18/HotFix/7.5.1.18.41/SDK/DBG

250 CWD command successful.

1. **bin**

ftp> bin

200 Type set to I.

1. **Get the files from this server**

ftp> mget \*

mget amdocs\_sdk\_ABP7.5.1.18.41\_64OG\_HP-UX.jar? y

200 PORT command successful.

150 Opening BINARY mode data connection for amdocs\_sdk\_ABP7.5.1.18.41\_64OG\_HP-UX.jar (46993951 bytes).

= bytes).

226 Transfer complete.

167 bytes received in 0.00 seconds (178.43 Kbytes/s)

**ftp> bye**